Propane Regulator Info

*We have had some customers experience weak flame on the stove and or the heater not staying lit, this is possibly due to your elevation.*

*We set all propane regulators to 11” water column here at the factory, this can be adjusted for your elevation.*

*Once you have checked the system IE: the tank valve is fully open to provide proper supply*

*This adjustment can be preformed by a certified propane shop.*